VERSION "FCB V1.0"


NS_ : 
	NS_DESC_
	CM_
	BA_DEF_
	BA_
	VAL_
	CAT_DEF_
	CAT_
	FILTER
	BA_DEF_DEF_
	EV_DATA_
	ENVVAR_DATA_
	SGTYPE_
	SGTYPE_VAL_
	BA_DEF_SGTYPE_
	BA_SGTYPE_
	SIG_TYPE_REF_
	VAL_TABLE_
	SIG_GROUP_
	SIG_VALTYPE_
	SIGTYPE_VALTYPE_
	BO_TX_BU_
	BA_DEF_REL_
	BA_REL_
	BA_DEF_DEF_REL_
	BU_SG_REL_
	BU_EV_REL_
	BU_BO_REL_
	SG_MUL_VAL_

BS_:

BU_: SCM PANEL
VAL_TABLE_ DM_ERR 1 "ERROR" 0 "NO_ERROR" ;
VAL_TABLE_ DM_LEVEL_TABLE 3 "LEVEL3" 2 "LEVEL2" 1 "LEVEL1" 0 "OFF" ;
VAL_TABLE_ DM_MOTOR_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_TABLE_ DM_KeyState 1 "PRESSED" 0 "NOT_PRESS" ;


BO_ 3221225472 VECTOR__INDEPENDENT_SIG_MSG: 0 Vector__XXX
 SG_ SCM_ERR_HEAT_SENSOR2 : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HEAT_SENSOR1 : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HALL_HG : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_OC_3 : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_OC_2 : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_OC_1 : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HALL_YT : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HALL_TZ : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HALL_ZY : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HALL_TT : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_HALL_KB : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_UV : 0|1@1+ (1,0) [0|0] "" Vector__XXX
 SG_ SCM_ERR_OV : 0|1@1+ (1,0) [0|0] "" Vector__XXX

BO_ 1030 SCM_DEBUG6: 8 SCM
 SG_ DEBUG_MOTOR_YT_HALLIO : 10|1@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_YT_STOP_2 : 48|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_YT_STOP_1 : 32|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_YT_STATUS : 8|2@1+ (1,0) [0|255] ""  PANEL
 SG_ DEBUG_MOTOR_YT_LOC : 16|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_YT_CURRENT : 0|8@1+ (1,0) [0|255] ""  PANEL

BO_ 1029 SCM_DEBUG5: 8 SCM
 SG_ DEBUG_MOTOR_TZ_HALLIO : 10|1@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TZ_STOP_2 : 48|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TZ_STOP_1 : 32|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TZ_STATUS : 8|2@1+ (1,0) [0|255] ""  PANEL
 SG_ DEBUG_MOTOR_TZ_LOC : 16|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TZ_CURRENT : 0|8@1+ (1,0) [0|255] ""  PANEL

BO_ 1028 SCM_DEBUG4: 8 SCM
 SG_ DEBUG_MOTOR_ZY_HALLIO : 10|1@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_ZY_STOP_2 : 48|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_ZY_STOP_1 : 32|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_ZY_STATUS : 8|2@1+ (1,0) [0|255] ""  PANEL
 SG_ DEBUG_MOTOR_ZY_LOC : 16|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_ZY_CURRENT : 0|8@1+ (1,0) [0|255] ""  PANEL

BO_ 1027 SCM_DEBUG3: 8 SCM
 SG_ DEBUG_MOTOR_TT_HALLIO : 10|1@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TT_STOP_2 : 48|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TT_STOP_1 : 32|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TT_STATUS : 8|2@1+ (1,0) [0|255] ""  PANEL
 SG_ DEBUG_MOTOR_TT_LOC : 16|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_TT_CURRENT : 0|8@1+ (1,0) [0|255] ""  PANEL

BO_ 1026 SCM_DEBUG2: 8 SCM
 SG_ DEBUG_MOTOR_KB_HALLIO : 10|1@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_KB_STOP_2 : 48|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_KB_STOP_1 : 32|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_KB_STATUS : 8|2@1+ (1,0) [0|255] ""  PANEL
 SG_ DEBUG_MOTOR_KB_LOC : 16|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_KB_CURRENT : 0|8@1+ (1,0) [0|255] ""  PANEL

BO_ 1025 SCM_DEBUG1: 8 SCM
 SG_ DEBUG_MOTOR_HG_HALLIO : 10|1@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_HG_STOP_2 : 48|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_HG_STOP_1 : 32|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_HG_STATUS : 8|2@1+ (1,0) [0|255] ""  PANEL
 SG_ DEBUG_MOTOR_HG_LOC : 16|16@1+ (1,0) [0|65535] ""  PANEL
 SG_ DEBUG_MOTOR_HG_CURRENT : 0|8@1+ (1,0) [0|255] ""  PANEL

BO_ 769 SCM_STATE: 8 SCM
 SG_ test5 : 56|8@1+ (1,0) [0|0] ""  PANEL
 SG_ test4 : 48|8@1+ (1,0) [0|0] ""  PANEL
 SG_ test3 : 40|8@1+ (1,0) [0|0] ""  PANEL
 SG_ test2 : 32|8@1+ (1,0) [0|0] ""  PANEL
 SG_ test1 : 24|8@1+ (1,0) [0|0] ""  PANEL
 SG_ ZY_MSSG_STATE : 20|2@1+ (1,0) [0|3] ""  PANEL
 SG_ ZY_HEAT_STATE : 18|2@1+ (1,0) [0|3] ""  PANEL
 SG_ ZY_FAN_STATE : 16|2@1+ (1,0) [0|3] ""  PANEL
 SG_ MOTOR_ZY_STATE : 10|2@1+ (1,0) [0|0] ""  PANEL
 SG_ MOTOR_YT_STATE : 8|2@1+ (1,0) [0|0] ""  PANEL
 SG_ MOTOR_TZ_STATE : 6|2@1+ (1,0) [0|0] ""  PANEL
 SG_ MOTOR_TT_STATE : 4|2@1+ (1,0) [0|0] ""  PANEL
 SG_ MOTOR_KB_STATE : 2|2@1+ (1,0) [0|0] ""  PANEL
 SG_ MOTOR_HG_STATE : 0|2@1+ (1,0) [0|0] ""  PANEL

BO_ 513 Panel_Key: 8 PANEL
 SG_ KEY_ZY_U : 1|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_ZY_MSSG : 20|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_ZY_HEAT : 17|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_ZY_FLAT : 32|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_ZY_FAN : 16|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_ZY_D : 0|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_YT_U : 9|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_YT_D : 8|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_TZ_U : 11|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_TZ_D : 10|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_TT_R : 2|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_TT_F : 3|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_RESET : 33|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_MEMORY_SET : 27|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_MEMORY_3 : 24|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_MEMORY_2 : 25|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_MEMORY_1 : 26|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_KB_R : 4|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_KB_F : 5|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_HG_R : 6|1@1+ (1,0) [0|0] ""  SCM
 SG_ KEY_HG_F : 7|1@1+ (1,0) [0|0] ""  SCM



CM_ BO_ 3221225472 "This is a message for not used signals, created by Vector CANdb++ DBC OLE DB Provider.";
BA_DEF_ EV_  "GenEnvIsGeneratedDsp" ENUM  "No","Yes";
BA_DEF_ EV_  "GenEnvAutoGenCtrl" ENUM  "No","Yes";
BA_DEF_ EV_  "GenEnvMsgOffset" INT 0 2147483647;
BA_DEF_ EV_  "GenEnvMsgName" STRING ;
BA_DEF_ EV_  "GenEnvIsGeneratedSnd" ENUM  "No","Yes";
BA_DEF_ SG_  "GenSigStartValue" FLOAT 0 1215752192;
BA_DEF_ SG_  "GenSigTimeoutValue" FLOAT 0 1215752192;
BA_DEF_ SG_  "GenSigInactiveValue" FLOAT 0 1215752192;
BA_DEF_ SG_  "GenSigMinValue" INT 0 2147483647;
BA_DEF_ SG_  "GenSigMaxValue" INT 0 2147483647;
BA_DEF_ SG_  "GenSigSendType" ENUM  "Cycle";
BA_DEF_ SG_  "GenSigEnvVarType" ENUM  "int","float","undef";
BA_DEF_ BO_  "GenMsgDelayTime" INT 0 0;
BA_DEF_ BO_  "GenMsgNrOfRepetition" INT 0 0;
BA_DEF_ BO_  "GenMsgCycleTimeFast" INT 0 0;
BA_DEF_ BO_  "NmMessage" ENUM  "No","Yes";
BA_DEF_ BO_  "GenMsgCycleTime" INT 0 65535;
BA_DEF_ BO_  "VFrameFormat" ENUM  "StandardCAN","ExtendedCAN","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","StandardCAN_FD","ExtendedCAN_FD";
BA_DEF_ BO_  "GenMsgSendType" ENUM  "Cycle";
BA_DEF_ BU_  "NmStationAddress" HEX 0 127;
BA_DEF_ BU_  "CANoeStartDelay" INT 0 0;
BA_DEF_ BU_  "CANoeDrift" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMin" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMax" INT 0 0;
BA_DEF_ BU_  "ECU" STRING ;
BA_DEF_ BU_  "NodeLayerModules" STRING ;
BA_DEF_  "BusType" STRING ;
BA_DEF_  "GenEnvVarPrefix" STRING ;
BA_DEF_  "GenEnvVarEndingSnd" STRING ;
BA_DEF_  "GenEnvVarEndingDsp" STRING ;
BA_DEF_  "DBName" STRING ;
BA_DEF_ BO_  "_Cdb_Sc_CTm_FAW_v3_0" INT 0 0;
BA_DEF_ BO_  "_Cdb_Sc_CTm_FAW_v2_3" INT 0 0;
BA_DEF_ BO_  "_Cdb_Sc_CTm_FAW_v3_1" INT 0 0;
BA_DEF_ BO_  "_Cdb_Sc_CTm_FAW_v2_2" INT 0 0;
BA_DEF_ BO_  "_Cdb_Sc_CTm_FAW_v2_1" INT 0 0;
BA_DEF_DEF_  "GenEnvIsGeneratedDsp" "No";
BA_DEF_DEF_  "GenEnvAutoGenCtrl" "No";
BA_DEF_DEF_  "GenEnvMsgOffset" 0;
BA_DEF_DEF_  "GenEnvMsgName" "";
BA_DEF_DEF_  "GenEnvIsGeneratedSnd" "No";
BA_DEF_DEF_  "GenSigStartValue" 0;
BA_DEF_DEF_  "GenSigTimeoutValue" 0;
BA_DEF_DEF_  "GenSigInactiveValue" 0;
BA_DEF_DEF_  "GenSigMinValue" 0;
BA_DEF_DEF_  "GenSigMaxValue" 0;
BA_DEF_DEF_  "GenSigSendType" "Cycle";
BA_DEF_DEF_  "GenSigEnvVarType" "undef";
BA_DEF_DEF_  "GenMsgDelayTime" 0;
BA_DEF_DEF_  "GenMsgNrOfRepetition" 0;
BA_DEF_DEF_  "GenMsgCycleTimeFast" 0;
BA_DEF_DEF_  "NmMessage" "No";
BA_DEF_DEF_  "GenMsgCycleTime" 0;
BA_DEF_DEF_  "VFrameFormat" "StandardCAN";
BA_DEF_DEF_  "GenMsgSendType" "Cycle";
BA_DEF_DEF_  "NmStationAddress" 0;
BA_DEF_DEF_  "CANoeStartDelay" 0;
BA_DEF_DEF_  "CANoeDrift" 0;
BA_DEF_DEF_  "CANoeJitterMin" 0;
BA_DEF_DEF_  "CANoeJitterMax" 0;
BA_DEF_DEF_  "ECU" "";
BA_DEF_DEF_  "NodeLayerModules" "";
BA_DEF_DEF_  "BusType" "CAN";
BA_DEF_DEF_  "GenEnvVarPrefix" "PE";
BA_DEF_DEF_  "GenEnvVarEndingSnd" "_Ps";
BA_DEF_DEF_  "GenEnvVarEndingDsp" "_Pd";
BA_DEF_DEF_  "DBName" "";
BA_DEF_DEF_  "_Cdb_Sc_CTm_FAW_v3_0" 0;
BA_DEF_DEF_  "_Cdb_Sc_CTm_FAW_v2_3" 0;
BA_DEF_DEF_  "_Cdb_Sc_CTm_FAW_v3_1" 0;
BA_DEF_DEF_  "_Cdb_Sc_CTm_FAW_v2_2" 0;
BA_DEF_DEF_  "_Cdb_Sc_CTm_FAW_v2_1" 0;
BA_ "DBName" "CanMatrix";
BA_ "NmStationAddress" BU_ PANEL 1;
BA_ "GenMsgCycleTime" BO_ 1030 50;
BA_ "GenMsgCycleTime" BO_ 1029 50;
BA_ "GenMsgCycleTime" BO_ 1028 50;
BA_ "GenMsgCycleTime" BO_ 1027 50;
BA_ "GenMsgCycleTime" BO_ 1026 50;
BA_ "GenMsgCycleTime" BO_ 1025 50;
BA_ "GenMsgCycleTime" BO_ 513 25;
VAL_ 3221225472 SCM_ERR_HEAT_SENSOR2 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HEAT_SENSOR1 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HALL_HG 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_OC_3 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_OC_2 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_OC_1 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HALL_YT 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HALL_TZ 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HALL_ZY 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HALL_TT 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_HALL_KB 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_UV 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 3221225472 SCM_ERR_OV 1 "ERROR" 0 "NO_ERROR" ;
VAL_ 769 ZY_MSSG_STATE 3 "LEVEL3" 2 "LEVEL2" 1 "LEVEL1" 0 "OFF" ;
VAL_ 769 ZY_HEAT_STATE 3 "LEVEL3" 2 "LEVEL2" 1 "LEVEL1" 0 "OFF" ;
VAL_ 769 ZY_FAN_STATE 3 "LEVEL3" 2 "LEVEL2" 1 "LEVEL1" 0 "OFF" ;
VAL_ 769 MOTOR_ZY_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_ 769 MOTOR_YT_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_ 769 MOTOR_TZ_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_ 769 MOTOR_TT_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_ 769 MOTOR_KB_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_ 769 MOTOR_HG_STATE 3 "FAULT" 2 "ACT_CCW" 1 "ACT_CW" 0 "NO_ACT" ;
VAL_ 513 KEY_ZY_U 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_ZY_MSSG 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_ZY_HEAT 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_ZY_FLAT 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_ZY_FAN 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_ZY_D 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_YT_U 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_YT_D 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_TZ_U 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_TZ_D 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_TT_R 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_TT_F 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_RESET 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_MEMORY_SET 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_MEMORY_3 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_MEMORY_2 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_MEMORY_1 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_KB_R 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_KB_F 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_HG_R 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 513 KEY_HG_F 1 "PRESSED" 0 "NOT_PRESS" ;

